(15) **Identifying inadequacies in existing risk controls according to the hierarchy of control and WHS legislative requirements.**

Elimination would be the first level of control and will be executed by eliminating the hazard at the source. For example, remove hazardous materials or abandon hazardous work practices.

Substitution will be the second level of control by substituting the hazard with something of lesser risk. For example, replace toxic materials with non-toxic materials.

Isolation: Isolate the hazard from the main work area. For example, store hazardous materials in a designated area away from where people are working.

Engineering controls: Us engineering controls to reduce the risk. For example, change equipment or tools being used, or install additional safety equipment.

Administrative controls will be the third and final control used in the hierarchy of control and will be executed by using administrative controls to lessen the risk. For example, introduce new work procedures and practices.

PPE: Use PPE. For example, provide and use hearing and eye protection, hard hats, gloves, masks and protective clothing such as coats and vests.